2011-2019 ZX10 OIL PAN INSTRUCTIONS

STEP 1... INSTALL STOCK OIL PAN GASKET TO BOTTOM OF MOTOR.
STEP 2… INSTALL STOCK PICK-UP RUBBER SEAL SAME AS REMOVED.
STEP 3… INSTALL STOCK RUBBER O-RING FROM STOCK PANS OIL TUBE FILTER OUTLET INTO BOTTOM OF MOTOR WITH FLAT SIDE OF SEAL AGAINST BOTTOM OF MOTOR AND ROUNDED SIDE TOWARD OIL PAN.  THIS O-RING IS REINSTALLED SAME AS IT WAS REMOVED.
STEP 4… NXS OIL PANS TOP SECTION CAN NOW BE MOUNTED TO BOTTOM OF THE MOTOR WITH TWO 1.75” SCREWS & ONE 1” SCREW.  DO NOT TIGHTEN SCREWS AT THIS TIME, HAND TIGHTEN 3 SCREWS ONLY. 
STEP 5… NXS SWIVEL PICK-UP NOW CAN BE INSTALLED. USE A LIGHT COAT OF OIL ON PICK-UP TUBE TO HELP SLIDE INTO PICK-UP TUBE RUBBER SEAL INSTALLED IN STEP 2.  A SLIGHT WIGGLE TO GET TUBE IN AND LINED UP WITH 2 MOUNTING HOLES WILL BE NEEDED.
STEP 6… TWO STAINLESS SCREWS WILL NEED SOME LOCTITE AND THEN INSTALLED THROUGH PICK-UP TUBE MOUNT AND INTO ITS MOUNTING HOLES AND THEN TIGHTEN THE TWO STAINLESS SCREWS SECURELY.
STEP 7… THREE SCREWS IN STEP 4 CAN NOW BE TIGHTENED.
STEP 8… REINSTALL STOCK CHECK VALVE INTO BOTTOM SECTION OF OIL PAN AND TIGHTEN SECURELY.
STEP 9… REUSE STOCK DRAIN TUBE REMOVING RUBBER HOSE.
STEP 10… NXS BOTTOM SECTION OF OIL PAN WILL COME WITH O-RING THAT WILL ALIGN WITH BOTTOM OF MOTOR OIL INLET.  APPLY A LIGHT COAT OF OIL ON O-RING.  THE BOTTOM SECTION WILL ALSO HAVE A LARGE THIN O-RING SEAL THAT SEALS THE TOP AND BOTTOM SECTION OF OIL PAN TOGETHER.  ALIGN THE TWO PARTS OF OIL PAN AND USING 3 SHORT SCREWS ATTACH BOTTOM OF PAN TO TOP OF PAN.  THEN USE 11 LONG SCREWS TO ATTCH COMPLETE PAN TO BOTTOM OF MOTOR.
STEP 11… WITH OIL PAN COMPLETE ON MOTOR TIGHTEN ALL SCREWS, BEING SURE NOT TO OVER TIGHTEN.
STEP 12… REUSE STOCK DRAIN PLUG AND TIGHTEN.    
                                   
                               QUESTIONS PH US AT 330-222-7061